Command Protocol

Issue 0.02

January 2015

Each command consists of 2 bytes.

First byte is the command, to or from the device.

Second byte is the data

|  |  |  |
| --- | --- | --- |
| **Function** | **Command** | **Data** |
| Relay Buttons | 0x90 | 0x10- 0x18. Set msb for On |
| LED Switches | 0x90 | 0x20-0x28. Set msb for On |
| Slide switches | 0x90 | 0x00-0x08. Set msb for on |
| PWM adjustment | 0x91 | 8 bit value to set |
| VR2 adjustment | 0x92 | 8 bit data |
| Set LCD Text | 0x71 | Line number, then data |
|  |  |  |
| Acknowledge | 0x74 | 0 for ACK, 1 for NAK |